**SPA PLUMBING CLEANSER**

It is recommended to cleanse the plumbing when:

1. You purchase a used spa or move into a home with a spa (use Awesome)
2. On a yearly basis to remove chemical build up (Spa marvel or Whirlpool Rinse)
3. If the spa is widely used by different people – social gatherings, holiday rentals/air B & B (Awesome or Spa Marvel).

**INSTRUCTIONS FOR USE**

1. Turn off all jets inside the spa and all diverters (control knobs).
2. Remove the filters, (this a good time to cleanse the filters overnight with the chemical filter cleaner, rinse and let dry before use for fiber pleats to regain natural form – suggested to have a second set to switch every 3 months)
3. Hit the jets/pumps to start circulation. Pour entire bottle of the Spa Marvel or Whirlpool Rinse but only **half** of the Awesome the hole of the filter assembly.
4. Circulate the spa for one full hour, leaving the cover off (after the 15 – 20 run cycle go back to press jet/pump option again – this will have to be done 3 -4 times)
5. Let spa run normally on its own for a minimum of 23 hours (you cannot use the spa during this time).
6. Drain spa as normal, wipe down with vinegar/water mix and refill.
7. Insert filters and “Happy Tubbing”

Enjoy!!